--- manual/s_phys_pkgs/text/fizhi.tex	2004/01/28 21:00:10	1.5
+++ manual/s_phys_pkgs/text/fizhi.tex	2004/02/02 22:00:18	1.6
@@ -888,3 +888,8 @@
 the model's moisture data is used.  Above 100 mb, the SAGE data is used.  Between 100 and 300 mb,
 a linear interpolation (in pressure) is performed using the data from SAGE and the GCM. 
 
+\subsection{Key subroutines, parameters and files}
+
+\subsection{Dos and donts}
+
+\subsection{Fizhi Reference}
