--- manual/s_examples/rotating_tank/tank.tex	2005/06/14 20:09:04	1.12
+++ manual/s_examples/rotating_tank/tank.tex	2010/08/30 23:09:20	1.18
@@ -1,4 +1,4 @@
-% $Header: /home/ubuntu/mnt/e9_copy/manual/s_examples/rotating_tank/tank.tex,v 1.12 2005/06/14 20:09:04 afe Exp $
+% $Header: /home/ubuntu/mnt/e9_copy/manual/s_examples/rotating_tank/tank.tex,v 1.18 2010/08/30 23:09:20 jmc Exp $
 % $Name:  $
 
 \bodytext{bgcolor="#FFFFFFFF"}
@@ -14,27 +14,26 @@
 %\end{center}
 
 \section{A Rotating Tank in Cylindrical Coordinates}
-\label{sect:eg-tank}
-\label{www:tutorials}
+\label{sec:eg-tank}
+%\label{www:tutorials}
 \begin{rawhtml}
 <!-- CMIREDIR:eg-tank: -->
 \end{rawhtml}
-
-This section illustrates an example of MITgcm simulating a laboratory
-experiment on much smaller scales than those commonly considered in  
-geophysical
-fluid dynamics.
+\begin{center}
+(in directory: {\it verification/rotating\_tank/})
+\end{center}
 
 \subsection{Overview}
-\label{www:tutorials}
+%\label{www:tutorials}
                                                                           
 This example configuration demonstrates using the MITgcm to simulate a
 laboratory demonstration using a differentially heated rotating
 annulus of water.  The simulation is configured for a laboratory scale
-on a $3^{\circ}$ $\times$ 1cm cyclindrical grid with twenty-nine
+on a $3^{\circ}\times1\mathrm{cm}$ cyclindrical grid with twenty-nine
 vertical levels of 0.5cm each.  This is a typical laboratory setup for
 illustration principles of GFD, as well as for a laboratory data
-assimilation project.
+assimilation project. The files for this experiment can be found in
+the verification directory under rotating\_tank.
 \\
 
 example illustration from GFD lab here
@@ -45,11 +44,11 @@
  
 
 \subsection{Equations Solved}
-\label{www:tutorials}
+%\label{www:tutorials}
 
 
 \subsection{Discrete Numerical Configuration}
-\label{www:tutorials}
+%\label{www:tutorials}
 
  The domain is discretised with a uniform cylindrical grid spacing in
 the horizontal set to $\Delta a=1$~cm and $\Delta \phi=3^{\circ}$, so
@@ -63,8 +62,8 @@
 something about heat flux
 
 \subsection{Code Configuration}
-\label{www:tutorials}
-\label{SEC:eg-baro-code_config}
+%\label{www:tutorials}
+\label{sec:eg-tank-code_config}
 
 The model configuration for this experiment resides under the
 directory {\it verification/rotatingi\_tank/}.  The experiment files
@@ -84,7 +83,7 @@
 to these files associated with this experiment.
 
 \subsubsection{File {\it input/data}}
-\label{www:tutorials}
+%\label{www:tutorials}
 
 This file, reproduced completely below, specifies the main parameters 
 for the experiment. The parameters that are significant for this configuration
@@ -210,14 +209,14 @@
 ($x,y,z$) map and is enumerated and formatted in the same manner as the 
 bathymetry file. 
 
-\item Lines 66 and 57
+\item Lines 66 and 67
 \begin{verbatim}
  tCylIn  = 0
  tCylOut  = 20
 \end{verbatim}
 These line specify the temperatures in degrees Celsius of the interior
 and exterior walls of the tank -- typically taken to be icewater on
-the inside and room temperature on the inside.
+the inside and room temperature on the outside.
 
 
 \end{itemize}
@@ -227,23 +226,23 @@
 notes.
 
 \begin{small}
-\input{part3/case_studies/rotating_tank/input/data}
+\input{s_examples/rotating_tank/input/data}
 \end{small}
 
 \subsubsection{File {\it input/data.pkg}}
-\label{www:tutorials}
+%\label{www:tutorials}
 
 This file uses standard default values and does not contain
 customizations for this experiment.
 
 \subsubsection{File {\it input/eedata}}
-\label{www:tutorials}
+%\label{www:tutorials}
 
 This file uses standard default values and does not contain
 customizations for this experiment.
 
 \subsubsection{File {\it input/thetaPol.bin}}
-\label{www:tutorials}
+%\label{www:tutorials}
 
 The {\it input/thetaPol.bin} file specifies a three-dimensional ($x,y,z$) 
 map of initial values of $\theta$ in degrees Celsius.  This particular 
@@ -251,7 +250,7 @@
 perturbations.
 
 \subsubsection{File {\it input/bathyPol.bin}}
-\label{www:tutorials}
+%\label{www:tutorials}
 
 
 The {\it input/bathyPol.bin} file specifies a two-dimensional ($x,y$) 
@@ -261,7 +260,7 @@
 in the same way as standard MITgcm two-dimensional, horizontal arrays.
 
 \subsubsection{File {\it code/SIZE.h}}
-\label{www:tutorials}
+%\label{www:tutorials}
 
 Two lines are customized in this file for the current experiment
 
@@ -280,18 +279,18 @@
 \end{itemize}
 
 \begin{small}
-\input{part3/case_studies/rotating_tank/code/SIZE.h}
+\input{s_examples/rotating_tank/code/SIZE.h}
 \end{small}
 
 \subsubsection{File {\it code/CPP\_OPTIONS.h}}
-\label{www:tutorials}
+%\label{www:tutorials}
 
 This file uses standard default values and does not contain
 customizations for this experiment.
 
 
 \subsubsection{File {\it code/CPP\_EEOPTIONS.h}}
-\label{www:tutorials}
+%\label{www:tutorials}
 
 This file uses standard default values and does not contain
 customizations for this experiment.
